09-10-14

Printed fitting with O-ring and 10-32 brass insert. Leak test by attaching low pressure (< 4 psi) air supply. Uses

Audio port under serial number label.



