Parts required for AT-Leakdown

1. Gauge – low pressure
2. Sealant
3. Manual Pump Bulb
4. Reservoir
5. Module fitting
6. Insert fitting
7. O-ring – 50 durometer
8. Air to Insert fitting
9. Tubing